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	TEST OF THE COMPRESSOR BLEED VALVE
TESTE DA VÁLVULA DE SANGRIA DO COMPRESSOR 



	ITEM
	PROCEDIMENTOS /TOLERÂNCIAS
	Condição
	Data
	Executante

	Item
	Procedures/Serviceable limits
	Condition
	Date
	Performed by

	1
	
Install bleed valve on bleed control gage fixture 6872546. (See Figure 6.)

	     
	     
	     

	2
	Adjust ambient pressure (Pa) to 14.7 psia (101 kPa) and apply a compressor discharge pressure (Pc) of 85.5 psia (572 kPa) and adjust the inlet and exit orifice size relationship to obtain an interstage pressure (Pi) of 36.6-37.8 psia (256-259 kPa) with the valve at the fully closed position. Record Pi. The fully closed position is defined as the touch of the valve to the valve seat.
	Pi:      
	     
	     

	3
	
Check remaining test points for Pi value specified.
 
	     
	     
	     



	Table 7
CALIBRATION LIMITS (P/N 23073207)

	Pa Psia
	Pc Psia
	Test Condition
	Pi Limits
Psia
	Pi
(Psia)

	
	
	
	Min
	Max
	

	14.7
	85.5
	Reducing (Pi) until Valve is just full closed**
	36.6
	37.8
	     

	14.7
	51.5
	Increasing (Pi) until Valve is just full open*
	20.3
	22.3
	     

	5.45
	34.0
	Reducing (Pi) until Valve is just full closed**
	13.5
	15.1
	     

	5.45
	19.0
	Increasing (Pi) until Valve is just full open*
	7.0
	8.7
	     

	** Full closed is defined as the touch of the valve to the valve seat.

	* Fully open is defined as a minimum open distance of at least 0.434 in. (11.02 mm).





	TEST DE VAZAMENTO
Leakage Test



	ITEM
	PROCEDIMENTOS /TOLERÂNCIAS
	Condição
	Data
	Executante

	Item
	Procedures/Serviceable limits
	Condition
	Date
	Performed by

	B
	Apply 125 psig (862kPag) of 21.1 ± 5°C (70 ± 9°F) air to the Pc port and 30 psig
(207kPag) of 21.1 ± 5°C (70 ± 9°F) air to the valve mounting Pi. Total leakage of Pc and
Pi shall not exceed 0.30 pound per minute.
	Total leakage: 

     
	     
	     

	C
	On units meeting service testing and location inspection and quality requirements, it is recommended that information pertinent to the following areas be reviewed and evaluated prior to re-lease of the unit for reinstallation on the engine.
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