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OVERHAUL MANUAL GTP5232-3 ATA 72-00-00 ENGINE TESTING

TR E3R22-72-1 – AUG. 12, 2022
	ENGINE STATUS
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	PERFORMANCE POINT
	TAKEOFF
	NORMAL CR.
	CRUISE A
	CRUISE B

	SPEC MGT (ºF)
	1423
	1325
	NA
	NA

	SPEC/PRED. SHP (HP)
	450/     
	380/     
	380/     
	317/     

	SPEC/PRED. SFC (lb/hr/HP)
	0.608/     
	0.631/     
	0.631/     
	0.666/     

	PERCENT DELTA FROM SPEC PWR (%)
	     
	     
	     
	     

	PERCENT DELTA FROM SFC (%)
	     
	     
	     
	     


	STARTS AND SHUTDOWN DATA

	TIME START

(HOURS)
	DATE

DD/MM/AA
	MGT MAX

°F
	TIME SHUTDOWN

(HOURS)
	FUEL USED

(LITERS)
	RUN TIME

(HOURS)

HH:MM
	REMARKS

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	     :     
	    /    /    
	     °F
	     :     
	     L
	     :     
	     

	
	TOTAL:
	     L
	        :     


	PRE- START CHECK LIST:

· Check test Cell Air Pressure. 

· Check the water inlet valve pressure its 1-1,8 psi. (20%)
· Check fuel Inlet Pressure. 
· Check starter enable.
· Check if vibration system is operating. 

· Check all temperatures and pressures, if is in accordance. 

· Reset max. values. 

· Check Master system its ON. 

· Check Oil Inlet valve is open. 

· Check Power Pack is ON. 

· Check oil level of dyno lubricating system.
· Check starter enable.

· Check Dyno system is operating in Speed Mode (6016 rpm in output shaft). 

NOTE: DO NOT START THE ENGINE IF THE MGT IS MORE THAN 302°F (150°C)


	COMPONENTS REPLACEMENT RECORD

	ITEM
	1
	2
	3

	DESCRIPTION
	     
	     
	     

	PN (REMOVED)
	     
	     
	     

	SN (REMOVED)
	     
	     
	     

	SN ENG. (REMOVED)
	     
	     
	     

	PN (INSTALLED)
	     
	     
	     

	SN (INSTALLED)
	     
	     
	     

	SN ENG. (INSTALLED)
	     
	     
	     

	DATE
	     /     /     
	     /     /     
	     /     /     

	APPROVED BY
	
	
	


	1
	Filter inspection:

Oil Filter:              

                         [image: image15.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image16.wmf]NOK


Fuel Filter:

                         [image: image17.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image18.wmf]NOK



	
	

	2
	Reset Fuel Flow Meters:

[image: image19.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image20.wmf]NOK



	
	

	3
	Select engine model C20J in Texcel VX 100                                         

[image: image21.wmf]OK


Check overspeed configuration                                                              

[image: image22.wmf]OK


Set inlet valve auto control values: 2.857(a) – 177,1(b).                    

[image: image23.wmf]OK



	
	

	4
	Inlet water valve pressure pump ½ open?

[image: image24.wmf]YES



	
	

	5
	Engine installed and checked.

[image: image25.wmf]OK



	
	

	6
	Perform FCU and PTG rigging

[image: image26.wmf]OK



	
	

	7
	Perform pre-start check list.
NOTE: DO NOT START THE ENGINE IF THE MGT IS MORE THAN 302°F (150°C)
	
	

	8
	Depreserve fuel system.


	
	

	9
	Do motoring and record bearing oil.

NOTE: RECORD OIL FLOW ON-SITE
#1           cc
    #6/7           cc
#8          _ cc
	
	

	10
	During the last motoring there was positive Main Oil Pressure?
[image: image27.wmf]YES



 CONTROL Forms.CheckBox.1 \s [image: image28.wmf]NO


	
	

	11
	Perform pre-start check list.
NOTE: DO NOT START THE ENGINE IF THE MGT IS MORE THAN 302°F (150°C)
	
	

	12
	Start engine, record MGT max.

NOTE: ALL START MUST BE RECORDED IN WORK INSTRUCTION PAGE 2. IF THE MOP NOT INCRESE WHEN N1 REACHES 10.000 RPM, STOP THE ENGINE. IF N2 NOT START TURN AT 20.000 RPM, SHUTDOWN THE ENGINE.
	
	

	13
	There was any problem during start or stabilization in Ground Idle? ​​​​​​

     
     
     

	
	

	14
	Main oil pressure is within the limits? (REF: 1 G (1) (b) 5)
N1 Speed
Minimum

Maximum

Within of limits?

Value

G.I. to 79%
50 psig

130 psig

[image: image29.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image30.wmf]NOK


      psig

79 to 94%
90 psig

130 psig

[image: image31.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image32.wmf]NOK


      psig

More than 94%
120 psig

130 psig

[image: image33.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image34.wmf]NOK


      psig
If not, adjust the Oil Pressure Regulating Valve adjustment. Item 1-G-(1)-(n).
	
	

	15
	Idle vibration is within the limits? 
Compressor:

                         [image: image35.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image36.wmf]NOK


Gearbox:

                         [image: image37.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image38.wmf]NOK


Turbine:

                         [image: image39.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image40.wmf]NOK



	
	

	16
	Setting 1 – Ground idle and Ground Start.
N1 speed is at 59 to 65%?                                                      

 [image: image41.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image42.wmf]NOK


NOTE: Record vibration in ground Idle. 
Seal Vent at Ground Idle:  _________ in.hg

 [image: image43.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image44.wmf]NOK



	
	

	17
	Oil inlet pressure is within the limits? (REF: 1 G (1) (b) 5)
Must be kept at 0-1,8 psig during engine operation
	
	

	18
	Perform on-site inspection of fuel, oil, and air leakage.
Air leakage 

     
[image: image45.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image46.wmf]NOK


Oil leakage 

     
[image: image47.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image48.wmf]NOK


Fuel leakage 

     
[image: image49.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image50.wmf]NOK



	
	

	19
	Flight Autorotation. (REF: 1 G (1) (b) 5)
Power turbine governor is in the position for 100% N2 (6016 RPN NP?) 
[image: image51.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image52.wmf]NOK


NOTE: RECORD VIBRATION IN FLIGHT IDLE.                     [image: image53.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image54.wmf]NOK


	
	

	20
	Perform Seal Break-in

NOTE: INLET VALVE MUST BE IN MANUAL MODE.
Engine is free of any abnormal noise and rubbing?
[image: image55.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image56.wmf]NOK


	
	

	21
	Setting 2 – Engine Shutdown
Stop Time N1           sec      N2          sec
	
	

	22
	Start engine.

NOTE 1: PERFORM PRE-START LIST BEFORE START

NOTE 2: ALL START MUST BE RECORDED IN WORK INSTRUCTION PAGE 2/9.

NOTE 3: DO NOT START THE ENGINE IF THE MGT IS MORE THAN 302 ºF (150ºC)
	
	

	23
	Setting 3 - Perform Vibration, Noise Scan.
NOTE: Record vibration log in flight Idle.                         

 [image: image57.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image58.wmf]NOK


Vibration at Takeoff:

 [image: image59.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image60.wmf]NOK


Torque:            lb.ft
TMOP:            psig
	
	

	24
	Setting 6 – Deceleration Check
Time from FCU lever movement to N1 reaches 35000 rpm:      sec

[image: image61.wmf]OK
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	25
	Setting 8 – Perform Power Calibration
NOTE: RECORD VIBRATION IN MAX. POWER.                  ( OK

( NOK
During the max power stabilization do a checks:
SOP
Min. 30 psig

Max. 40 psig

            psig
[image: image63.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image64.wmf]NOK


Seal vent

 Max. 10 in.Hg
      in.Hg
[image: image65.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image66.wmf]NOK


RGB static

Refer to Appendix A (fig. 701)
      in.H2O
[image: image67.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image68.wmf]NOK


Power Fluctuation
Must not be more than +/- 250RPM

	
	

	26
	Setting 4 – Anti Ice.
GPTOT and anti-ice temperature rises?                        
 [image: image69.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image70.wmf]NOK


N1 and torque decreases?                                               

 [image: image71.wmf]OK
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	27
	Setting 5 – Governor Droop Check

 [image: image73.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image74.wmf]NOK



	
	

	28
	Setting 7 – Acceleration Check
Calculate 65% of torque value from setting 3:            lb.ft

Calculate 95% of TMOP value from setting 3:             psig

The acceleration time:       sec

Within acceptable limits?                                              

 [image: image75.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image76.wmf]NOK



	
	

	29
	Engine Shutdown
Checks if rotors are free of any locking.                      

[image: image77.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image78.wmf]NOK


Checks if there was smoke during the shutdown.     

[image: image79.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image80.wmf]NOK


Checks noises and rubbing of engine until the rotors stop

[image: image81.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image82.wmf]NOK


Record Stop Time: N1           sec/        N2           sec
	
	

	30
	Setting 8 – Calculate a Power Calibration

[image: image83.wmf]Acceptable
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	31
	Seal vent validation
With seal vent pressure within limits in max power, check no indication of oil vapor or leakage.

Record orifice:      
Record breather leakage       drops/min
	
	

	32
	Perform smoke test if applicable:
 [image: image85.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image86.wmf]NOK



 CONTROL Forms.CheckBox.1 \s [image: image87.wmf]NA


	
	

	33
	Compressor Vibration Reports. 

Compressor Vib. within parameters?
 MAX Transient           ips / MAX Steady           ips

(0,6 in/sec STEADY STAGE; 1,2 in/sec TRANSIENT max 6 sec)
[image: image88.wmf]YES



 CONTROL Forms.CheckBox.1 \s [image: image89.wmf]NO


	
	

	34
	Gearbox Vibration Reports.

Gearbox Vib. within parameters? 
 MAX Transient           ips / MAX Steady           ips 
(0,6 in/sec STEADY STAGE; 1,2 in/sec TRANSIENT max 6 sec)
[image: image90.wmf]YES



 CONTROL Forms.CheckBox.1 \s [image: image91.wmf]NO


	
	

	35
	Turbine Vibration Reports.

Turbine Vib. within parameters?
 MAX Transient           ips / MAX Steady           ips 
(0,9 in/sec STEADY STAGE; 1,8 in/sec TRANSIENT max 6 sec)
[image: image92.wmf]YES
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	36
	Perform fuel system preservation.

[image: image94.wmf]YES
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	37
	Filter inspection
Oil filter:      

 [image: image96.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image97.wmf]NOK


Fuel filter:   

 [image: image98.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image99.wmf]NOK


Replace fuel filter packings:           
[image: image100.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image101.wmf]NOK



 CONTROL Forms.CheckBox.1 \s [image: image102.wmf]NA



	
	

	38
	Chip detectors inspection.
[image: image103.wmf]OK



 CONTROL Forms.CheckBox.1 \s [image: image104.wmf]NOK


Replace chip detectors packings           
 [image: image105.wmf]OK
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 CONTROL Forms.CheckBox.1 \s [image: image107.wmf]NA


	
	

	39
	Drain RGB and record amont of oil.
NOTE: RECORD IN OIL FLOW CHECK ON-SITE TEST CELL

           ml (650ml max)
	
	

	40
	Remove the dressing kit and fit blank the engine.
	
	

	41
	Send engine and documentation workshop.
	
	


	REMARKS:

	

	TEST CELL OPERATOR:    
	DATE:
	TEST CELL INSPECTOR:
	DATE:
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