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	CUIDADO: INSPECIONAR O ANEL DE RETENÇÃO ANTES DA INSTALAÇÃO PARA CERTIFICAR QUE ESTE NÃO TEM DEFEITO E APÓS A INSTALAÇÃO PARA CERTIFICAR SE ESTÁ ASSENTADO CORRETAMENTE.
(1) Instalar os componentes do filtro de bypass, incluindo a poppet, mola, o anel lubrificado e o guia, no alojamento do filtro. Reter os componentes no alojamento com um anel de retenção interno. Usar o dispositivo 6798807 para facilitar a instalação do anel de retenção.
CAUTION:   INSPECT THE RETAINING RING BEFORE INSTALLATION TO BE SURE IT HAS NO DEFECTS AND AFTER INSTALLATION TO BE SURE IT IS PROPERLY SEATED.
(1) Install the filter bypass components, which include the poppet, spring, lubricated packing andguide, in the filter housing. Retain components in housing with an internal retaining ring. Use 6798807 compressor to aid in installation of the retaining ring.
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	(2) Lubrificar e instalar o anel no guia do regulador de pressão. Inserir a poppet, mola e guia dentro do alojamento do filtro. Fazer um ajuste aproximado do regulador pelo topo e ajustar o parafuso de ajuste retrocedendo 5 ½ voltas.
(2) Lubricate and install the packing on the pressure regulator guide. Insert poppet, spring, and guide into the filter housing. Make an approximate adjustment of the regulator by bottomingthe adjusting screw and backing out 5 ½ turns.
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	(3) Testar o alojamento do filtro de óleo como segue:
(a) Plugar o tubo vertical de pressão e instalar o tampão no alojamento do filtro.
(b) Conectar uma fonte de líquido de calibração de (24 – 29 °C) ou óleo de motor (82 °C), na entrada do alojamento do filtro, temperatura aplicada (________) °C.
(3) Test the lube oil filter housing as follows:
(a) Plug the standpipe and install the cap on the filter housing.
(b) Connect a supply of calibration fluid at (24 – 29°C) or engine oil at (82°C) to the filter housing inlet port.
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	(c) Lentamente aumentar a pressão aplicada até a válvula by-pass abrir. A pressão deve estar de 80 – 130 psig, aplicada (________) psig.
(d) Diminuir a pressão para 30 psig. Vazamentos através da válvula de by-pass não devem exceder a 63 cc por minuto, encontrado (________) cc.
(e) Conectar a fonte de fluído na saída e tamponar a entrada.
(f) Ajustar a fonte de suprimento de fluído para obter um fluxo de 720 pph através da válvula reguladora de pressão, encontrado (________) pph.
(g) Ajustar o conjunto do guia até 130 ± 5 psig ser obtido com 720 pph de fluxo. Pressão (________) psig e fluxo (________) pph encontrados.
(h) Diminuir o fluxo para 20 pph. A pressão não deve ser menor que 130 ± 5 psig. Fluxo (________) pph e pressão (________) psig encontrados. Se a pressão não ficar dentro dos limites, repetir os passos (f) e (g), ajustando o conjunto guia para uma pressão mais elevada entre 130 ± 5 psig. Se a pressão for menor que 125 psig a 20 pph, substituir a válvula poppet reguladora de pressão e repetir o teste inteiro.
(i) Remover o tampão e o plugue do tubo vertical de pressão. Remover o plugue da entrada.
(c) Slowly apply increasing pressure until the bypass valve opens. Pressure must be 80 – 130 psig.
(d) Decrease pressure to 30 psig. Leakage through the bypass valve must notexceed 63 cc per minute.
(e) Connect the fluid supply to the outlet port and plug the inlet port.
(f) Adjust the fluid supply to obtain a flow of 720 pph (326kg/hr) across the pressureregulator valve.
(g) Adjust the guide assembly until 130  5 psig is obtained with 720 pph flow.
(h) Decrease flow to 20 pph. Pressure must not be less than 130 ± 5 psig. If pressure is not within limits, repeat steps (f) and (g), adjusting the guide assembly for a higher pressure within the 130  5 psig range. If pressure is less than 125 psig at 20 pph, replace the pressure regulating poppet valveand repeat the entire test.
(i) Remove the cap and remove the plug from the standpipe. Remove the plug from the inlet port.
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	(4) Instalar o conjunto do filtro com anel no alojamento do filtro. Instalar o tampão com um anel lubrificado no alojamento do filtro. Fixar o tampão com 2 porcas e 2 arruelas. Torquear as porcas de 35 – 40 lb.in, aplicado (________) lb.in.
(4) Install the filter assembly with packing in the filter housing. Install the cap with lubricated packing on the filter housing. Secure the cap with two nuts and washers. Torque nuts to 35 – 40 lb.in.
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	NOTA
NOTE
	Se um indicador de filtro de óleo for usado, torqueie de 100 – 125 lb.in e frene
If an oil filter indicator is used, then tighten to 100 – 125 lb.in. and lockwire.
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