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	Operação
Sequence
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	1
	Pag. 1009
1.(G).(3)
	(i). Balancear o gas producer turbine rotor (72-51-00-01-115) como descrito abaixo:
Assemble and balance the gas producer turbine rotor assembly (72-51-00-01-115) as matched sets (Ref. FIG. 1018) as follows: 
2 Balancear o gas producer turbine rotor com uma tolerância de 1,44 mg. m (Ref. FIG. 1018, AXIS H).
Balance the gas producer turbine rotor with a tolerance of 1,44 mg. m. (Ref. Fig. 1018, Axis H).
Inicial LH (     ) mg.m			Inicial RH (     ) mg.m
	     
	     

	2
	
	(i). Balancear o gas producer turbine rotor (72-51-00-01-115) como descrito abaixo:
Assemble and balance the gas producer turbine rotor assembly (72-51-00-01-115) as matched sets (Ref. FIG. 1018) as follows: 
2 Balancear o gas producer turbine rotor com uma tolerância de 1,44 mg. m (Ref. FIG. 1018, AXIS H).
Balance the gas producer turbine rotor with a tolerance of 1,44 mg. m. (Ref. Fig. 1018, Axis H).
  Final LH (     ) mg.m			Final RH (     ) mg.m
	     
	     

	NCC
	Data Validade|Expiration Date

	BALANCEADORA SCHENK HORIZONTAL NCP: 000286
SCHENK HORIZONTAL BALANCER NCP: 000286
	     /     /     
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